A UNIX System Implementation for System/370*

W. A. FELTON, G. L. MILLER, and J. M. MILNER

ABSTRACT

This paper describes an implementation of the UNIX(TM) operating system for IBM Sys-

tem/370 computers. In this implementation an underlying Resident Supervisor, adapted

from an existing IBM control program, provides machine control and multiprogramming;

while a UNIX System Supervisor, adapted from the standard UNIX system kernel, pro-

vides the UNIX system environment. This implementation supports multiprocessing,

paging, and large-process, virtual address spaces. Terminal handling is done through an

outboard terminal processor. This paper describes the software structure, with emphasis

on unique aspects of this implementation: multiprocessing and process synchronization,

process creation, and outboard terminal handling. Capacity and performance of the

UNIX system on large mainframes is also discussed. The first and principle user of the

UNIX system for System/370 is the development project for the 5ESS(TM) switching

system. This paper also discusses the use of a large mainframe UNIX system for this

development. Included in this discussion are the reasons for selecting this system for

development, applications software porting, and general experience with mainframe

UNIX systems.

I. INTRODUCTION

One of the great strengths of the UNIX operating system is its portability. UNIX system implementa-

tions have been done for a variety of computers with greatly varying architectures [1]. Perhaps nowhere is

this portability better illustrated than in its implementation for System/370 machines.

Since its introduction by IBM in 1970, System/370 [2] has become the dominant architecture for

large computer systems; currently about 70 percent of the large mainframes in the United States follow

System/370 architecture. IBM builds a variety of System/370 machines, from relatively small "superminis"

to their largest processors. In addition, other manufacturers, such as Amdahl Corporation, build machines

that conform to System/370 specifications and can thus run System/370 operating systems and applications.

The principal operating system currently used on these machines is IBM’s MVS (Multiple Virtual System),

although other operating systems--IBM’s VM/370 and TSS/370, and the University of Michigan’s MTS--

are also available.

The idea of a UNIX system implementation on System/370 machines, which would bring the power

of these large processors to the UNIX system user, has been discussed for some time. In 1978 we began to

seriously study the possibility of such an implementation. Our primary objective was to develop a true ver-

sion of the UNIX operating system that would be suitable for use in a production environment on Sys-

tem/370 machines, making full use of the features and power of these large machines. We wanted to make

the System/370 environment appear to the user and applications programmer as similar as possible to the

standard UNIX system environment; in the words of one developer, it should "look, feel, and smell like the

UNIX system people are familiar with". At the same time, we wanted a system that would provide reliable,

cost-effective production service, as, for example, in a computation center environment. Most of the design

for implementing the UNIX system for System/370 was done in 1979, and coding was completed in 1980.

The first production system, an IBM 3033AP, was installed at the Bell Laboratories facility at Indian Hill in

early 1981. Since then several large IBM System/370 mainframes have been made to run the UNIX system

at Indian Hill. In addition, there are installations at Holmdel and Denver.

The first user of the UNIX system for System/370, and currently the largest user, is the development

__________________

Published in, and copyright by, AT&T Bell Laboratories Technical Journal, Vol. 63, No. 8 Part 2, October 1984. Photore-

production for noncommercial use is permitted without payment of royalty provided that each reproduction is done without

alteration and that the Journal reference and copyright notice are included on the first page.

- 2 -

project for the 5ESS switch. Even as the system was being developed, the needs of the project were quickly

reaching beyond the use of minicomputers. The UNIX operating system was selected as the development

system to be used by the programmers developing the switching system software. The UNIX system was

selected because of the facilities of the Programmer’s Workbench [4] software, which provide the develop-

ers with editors, source code control, and software generation systems. Initially, development was done on

several PDP-11/70 systems. By late 1980 the project was using nine PDP-11/70 systems to provide the

programmer development support environment. These computers were linked together using a commer-

cially available high-speed network with drivers written for the UNIX operating system. The fragmentation

of the project over nine computers caused significant additional work. The low-level compiled objects that

were compiled on the nine computers had to be networked onto one computer for the final linking before

generating the final switching program output. The final products had to be distributed back to the other

eight computers so that private changes could be linked into the full system for private testing. Also, peri-

odic auditing had to be done to ensure that all computers had the same common data and that the compilers

and other tools remained the same on each system. The project was continuing to grow, and adding more

minicomputers was not the best solution, because the auditing and networking overhead would increase on

all the minicomputer systems.

Several solutions were considered to the problem of the growing number of minicomputers required

for the project. The UNIX operating system with the Programmer’s Workbench software provided a better

development environment than any other operating system available. In addition, the developers were all

trained in using this system and all the software tools had been developed. This led to a requirement that the

computer systems selected to solve the problem support the UNIX operating system, as well as provide an

order of magnitude more computing power in one system than the PDP-11/70 systems that were being

used. This requirement ruled out larger minicomputers such as the VAX-11/780 systems, which offers

approximately twice the computing power of the PDP-11/70 system. The IBM 3033AP processor met the

requirement with approximately 15 times the computing power of a single PDP-11/70 processor. After

studying the problem, the project decided to use the UNIX system for System/370, and requested that the

porting be completed and a production grade system be made available in mid-1981.

II. SOFTWARE ENVIRONMENT

We initially thought about porting the UNIX operating system directly to System/370 with minimal

changes. Unfortunately, there are a number of System/370 characteristics that, in the light of our objectives

and resources, made such a direct port unattractive. The Input/Output (I/O) architecture of System/370 is

rather complex; in a large configuration, the operating system must deal with a bewildering number of

channels, controllers, and devices, many of which may be interconnected through multiple paths. Recovery

from hardware errors is both complex and model-dependent. For hardware diagnosis and tracking, cus-

tomer engineers expect the operating system to provide error logs in a specific format; software to support

this logging and reporting would have to be written. The System/370 architecture lends itself to the use of

paging for memory management; the UNIX system used swapping. Finally, several models of System/370

machines provide multiprocessing, with two (or more) processors operating with shared memory; the

UNIX system did not support multiprocessing.

Since code to support System/370 I/O, paging, error recording and recovery, and multiprocessing

already existed in several available operating systems, we investigated the possibility of using an existing

operating system, or at least the machine-interface parts of one, as a base to provide these functions for the

System/370 implementation. We needed a well-structured system that could provide a clean interface for

UNIX system processes. The system would have to provide all the functions needed by UNIX system pro-

cesses, or at least be extendible to provide these functions with reasonable effort.

Of the available systems, TSS/370 came the closest to meeting our needs and was thus chosen as the

base for our UNIX system implementation [5]. The choice of TSS/370 was a controversial one; it is a little

known and inadequately documented system. Still, it came the closest to providing the structure and func-

tion needed to support UNIX system processes, and it appeared that it could be enhanced to provide any

missing functions with reasonable effort. In 1979 we proposed to IBM that they make the necessary modifi-

cations to the TSS supervisor to support UNIX system processes, according to our design. IBM agreed to

do so under a program license agreement, and the first version of the enhanced TSS was delivered in 1980.

- 3 -

2.1 Software structure

The UNIX system for System/3 70 comprises three classes of programs, running in different software

levels. From highest to lowest, these are:

1. User-level programs, including user-written programs and system-provided programs, such as the

shell;

2. The UNIX System Supervisor, which incorporates much of the function and C-language code of the

standard UNIX system kernel; and

3. The Resident Supervisor, which supports the multiprogramming of UNIX system processes, provides

low-level system calls, and manages the physical system configuration.

Each UNIX system process, comprising a user-level program and the UNIX System Supervisor, exe-

cutes within its own 16-megabyte virtual memory, in the context of its own virtual machine. The Resident

Supervisor controls the resources allocated to these virtual machines, including process scheduling, dis-

patching, and real storage management.

User programs and the UNIX System Supervisor share the same 16-megabyte process space. The

UNIX System Supervisor is located in the upper 8 megabytes of this space; user programs are located in the

lower 8 megabytes. "Page 0", the lowest 4096 bytes of the process space, is reserved for Program Status

Words (interrupt vectors) and other information associated with the process virtual machine. The Sys-

tem/370 protection mechanism is used to prevent user-level program access to the UNIX System Supervi-

sor. The System/370 architecture allows sharing segments among several virtual memories; as in the stan-

dard UNIX system, this facility is used to permit sharing both read-only user text and UNIX System Super-

visor itself among UNIX system processes.

A program in one level communicates with the next lower level through system calls. There are two

types of system calls: UNIX system calls, as defined by the UNIX System User Reference Manual, used by

user-level programs to invoke the UNIX System Supervisor; and Resident Supervisor system calls, used by

the UNIX System Supervisor to request certain lower-level functions of the Resident Supervisor. User-level

programs never communicate directly with the Resident Supervisor. Information may be passed from a

lower level to the next higher level either synchronously as return data from a system call, or asyn-

chronously as a virtual machine interrupt (Resident Supervisor to UNIX System Supervisor) or a signal

(UNIX System Supervisor to user-level program). Where available, the system takes advantage of the Sys-

tem/370 Virtual Machine Assist feature, which allows a user-level system call to be passed directly to the

virtual machine.

2.2 Paging

As with most System/370 operating systems, the UNIX system for System/370 uses paging to man-

age main storage. A 16-megabyte process consists of up to 4096 pages, each of 4096 bytes; only those

pages that have been allocated and referenced by the process physically exist. At any given time, these

pages may be scattered through main storage and secondary (drum or disk) storage. For each process, the

Resident Supervisor maintains segment and page tables, giving the main and secondary storage locations of

its pages; these tables are used by the hardware when translating a virtual address to a physical main storage

address. Pages are brought into main storage on demand; when an executing process attempts to reference a

page not in main storage, a page fault occurs. The Resident Supervisor initiates an input operation to bring

the missing page from secondary storage to main storage. The process is blocked while the page is read,

and another process may be given the processor. The fact that a process may be arbitrarily blocked by a

page fault while executing in the UNIX System Supervisor has ramifications to process synchronization;

this is discussed in Section 2.5.

Process pages are moved out of main storage to secondary storage as necessary, on a roughly least

recently referenced. The Resident Supervisor attempts to keep the "working set" of active processes-- those

pages recently referenced--in main storage. All of a process’ pages, including those containing the UNIX

System Supervisor, are paged; a process that has been inactive for some time has no pages left in main stor-

age. In addition, the process segment and page tables themselves can be paged and will also eventually be

moved to secondary storage if the process is long inactive. The amount of permanently resident informa-

tion required to represent a process is quite small, a few hundred bytes. The system also has a page

- 4 -

migration mechanism, whereby pages of long-inactive processes may be moved from fast secondary stor-

age (drum, fixed-head disk, or solid-state memory) to slower storage (moving-head disk).

2.3 I/O system

UNIX file systems on System/370 are in format identical to standard UNIX file systems, except that

the block size has been enlarged to 4096 bytes. This block size is more appropriate to a larger system and

allows us to use the paging interface described in this section. As in the standard UNIX system, I/O is

blocked through a large number of block buffers, which effectively form a cache memory for recently refer-

enced blocks. These buffers exist in shared virtual memory within the UNIX System Supervisor area. On a

16-megabyte system, we typically allocate 4 megabytes to block buffers. When a block I/O request is made

to the UNIX System Supervisor, it first searches this cache for the desired block. If the block is not found, it

allocates a buffer for the block and asks the Resident Supervisor to read it in.

The Resident Supervisor provides simple read block and write block primitives, which

essentially provide a UNIX System Supervisor interface to the Resident Supervisor’s paging mechanism.

Requests for file system I/O from the UNIX System Supervisor are handled in essentially the same way as

paging requests initiated by the Resident Supervisor. For example, a read block request simply updates

the process page table. The block may not actually be read until the UNIX System Supervisor attempts to

reference it, at which point a page fault occurs and the input operation is processed like a normal page-in

operation. The UNIX System Supervisor may also request that I/O be initiated at the time a read block

is executed; this is usually done to provide I/O and process execution overlap. All disks and drums in the

System/370 configuration are formatted into 4096-byte records. All I/O to these devices is done through

highly optimized "drivers" in the Resident Supervisor. Storage on these devices may be allocated either to

the Resident Supervisor for process paging, or the the UNIX System Supervisor for file system storage.

The Resident Supervisor’s read block primitive is used by the UNIX System Supervisor in a spe-

cial way when processing an exec system call. Rather than reading the executable file into main storage

through the buffer cache, the Resident Supervisor effectively maps the executable file into the lower part of

the UNIX system process virtual address space by putting pointers to the file’s disk blocks in the process

page tables. As this program executes, the usual page-fault mechanism is used to read missing blocks of the

executable file into main storage. The advantage of this mechanism is that only those blocks of an exe-

cutable file that are actually required during execution are read into main storage.

The function and form of the character I/O system is conventional. Most drivers for character-

oriented devices construct channel programs styled after System/370, and issue the Resident Supervisor

iocall system call to execute them. All devices are known symbolically to the UNIX System Supervi-

sor; the Resident Supervisor does the messy work of translating the symbolic address into a physical

address, finding a nonbusy path to the device (including a different processor in some configurations), and

initiating physical I/O. Terminal device drivers work through a special terminal interface to a front-end

processor; this is discussed in Section 2.6.

2.4 Process creation

As in the standard UNIX system, processes are created by the fork system call; the new (child) pro-

cess is created by effectively copying the calling (parent) process. In the System/370 implementation, a

conventional fork would be complicated by the fact that parts of the parent process may be scattered

through main and secondary storage. Since the user process may be very large (nearly 8 megabytes), a full

copy could also be very slow.

Fortunately, we can again take advantage of the page-fault mechanism to avoid explicitly copying

except when necessary, and to delay most of this copying so as to minimize the data actually copied at the

time a fork is executed. When a child is created, both the child and parent’s page tables are set to point to

the same copy of a page--be it in main or secondary storage--with the "page fault" bit set. A private page

that is "temporarily" assigned to both a parent and a child is called a multiplexed page, and a multiplexed

page count, the count of processes that own this page, is kept. Subsequently, if either the parent or the child

references this page, a page fault occurs; at this time the page is actually copied, and the multiplexed page

count is decremented. Whenever the multiplexed count is reduced to one--either due to copying, or because

the parent or child releases the page due to process death or an exec --the page is no longer considered to

- 5 -

be multiplexed and may be given directly to the remaining process. In practice, this multiplexed page

mechanism is quite efficient, because it implicitly takes advantage of a common UNIX system characteris-

tic. In most cases, following a fork system call, the child process almost immediately performs exec on

another program, thus discarding the data just copied by fork . By not copying most process data until

those data are actually referenced--which, in the usual case, never happens--the System/370 fork executes

rapidly, regardless of process size.

1.5 Process synchronization

In the standard UNIX system, process synchronization is achieved through events with associated

sleep and wake-up operations. This mechanism is adequate for the usual UNIX system environment, in

which processes cooperatively share a single processor. This mechanism is not sufficient for the Sys-

tem/370 implementation, for two reasons. First, a process on the System/370 may be arbitrarily blocked by

the Resident Supervisor at any time (for example, because of a page fault), and another process be given the

processor. Second, several models of System/370 are multiprocessors, with two or more identical proces-

sors sharing a common main storage and, in some cases, a common I/O configuration. In such a system, we

may have two or more processes executing at the same time, possibly executing the same UNIX System

Supervisor instructions. We thus need a synchronization mechanism that is indivisible on a single proces-

sor and that guarantees synchronization when simultaneously executed on a multiprocessor.

Perhaps the best known process synchronization mechanism is the Dijkstra semaphore, with associ-

ated P and V operations. A semaphore is simply a counter. When positive, it represents the number of

resources available (typically, one when used for mutual exclusion); when negative, its absolute value is the

number of processes waiting for the resource. The P operation is used to obtain the resource; it decrements

the counter and waits if necessary. The V operation is used to release the resource; it increments the counter

and awakens the (next) waiting process, if any. Semaphores have the desired indivisibility and

multiprocessor-synchronizing properties, and in most cases replacing sleep and wake ups with P and V,

respectively, was straightforward.

However, simply replacing existing events with semaphores is not sufficient. In the standard UNIX

system, the kernel uses synchronization only where there is some possibility that it may have to give up the

processor-typically to wait for an I/O operation to complete. In the System/370 implementation we must

guarantee exclusive access to virtually all updates of shared system data by the UNIX System Supervisor.

We thus had to identify all instances of such updates in the UNIX System Supervisor and surround them

with P and V operations.

Extending process synchronization to all shared data objects in the UNIX System Supervisor was one

of the more difficult parts of this implementation. This had to be done so as to guarantee the validity of the

data, while avoiding the possibility of race conditions and lockouts. To minimize process blockage, we

wanted this synchronization to be fine-grained-for example, to protect individual elements in an array or

table, rather than simply the whole table. This led to a large number of semaphores, with rules concerning

how and in what order P and V operations should be executed. Happily, the basic structure of the UNIX

system kernel lent itself to this effort; very few changes in structure or program flow were made.

The System/370 instruction set does not contain P and V instructions. However, it does include a

synchronizing instruction, Compare and Swap (CS), that was used in implementing P and V. The efficiency

of P and V is critical; most file-system system calls execute a dozen or more of these operations. We were

able to implement these operations in such a way that the Resident Supervisor is called for a P operation

only if the process must wait, and for a V operation only if another process is waiting. Initially, P and V

were implemented as assembler-language subroutines; subsequently they were reimplemented as inline

macros. A side benefit of semaphores, especially significant on larger processors with many processes, is

that only one process-the next in line-is awakened by the V operation; in essence the process executing the

V passes control of the resource to the next waiting process. This differs from event synchronization, in

which all processes waiting for the event are awakened by wake-up, and must again compete for the

resource.

- 6 -

2.6 Terminals

One of the more difficult problems in making the System/370 environment look like the standard

UNIX system environment occurred in terminal handling. The standard UNIX system uses a full-duplex

protocol: characters typed by a user at the terminal are not displayed immediately but are sent to the proces-

sor; they are (usually) reflected back and printed or displayed. A user program may choose to process each

character as it comes in ("raw mode"). Large IBM systems conventionally use a half-duplex protocol: char-

acters are printed or displayed by the terminal as they are typed and sent to a communications controller.

The characters are usually buffered here and not sent to the main processor until a special signal or charac-

ter (e.g., carriage return) is typed. The UNIX system is considerably more flexible, in that special characters

and associated functions can easily be defined by system or user software. However, it does imply the over-

head of an I/O interrupt with each character. Some systems, such as the AT&T 3B20S computer, avoid this

overhead in normal operation with a special I/O or front-end processor.

In the System/370 implementation, we wanted to provide full-duplex terminal protocol with standard

UNIX system features but without character-at-a-time interrupts in the usual case. This implied the use of a

front-end processor tailored to the UNIX system environment. The standard IBM System/370 communica-

tions controllers proved unsuitable for this application. However, IBM makes a minicomputer, the Series/1,

with both good terminal communications facilities and a System/370 channel interface. Further, there were

existing Series/1 control programs that could be used as a base for a UNIX system terminal handler. Conse-

quently, we contracted with IBM’s General Systems Division to provide a UNIX system terminal handler

to our specifications. This code was delivered in late 1980, and the Series/1 is currently used for terminal

handling on the System/370.

We have recently implemented a prototype front-end processor for the UNIX system for System/370

using a 3B20S system running standard UNIX System V. This implementation has a number of advantages;

for example, it allows us to provide all the terminal features offered on the 3B20S computer in System V

and subsequent releases. Also, it may eventually allow us to down load some frequently used character-

oriented, raw-mode programs, such as screen editors, from the System/370 host. Although initially imple-

mented on a 3B20S computer, other models in the 3B family of computers may be used. A number of such

processors linked together with a System/370 mainframe could form a network of individual and group

work stations, providing access to the powerful central machine as needed.

III. PERFORMANCE

One of the most interesting questions about the UNIX system on System/370 is its performance. A

number of factors made the performance of the System/370 implementation unique. These factors have a

considerable impact on the performance trade-offs made in the typical minicomputer implementations of

the UNIX system. Coupled with the computing requirements of the large system-development task for

which it was first used, the 5ESS local digital switch, these factors determined the capacity of the Sys-

tem/370 implementation. The scale of the system also demands longer-range capacity forecasting than typi-

cally applied in minicomputers. The following sections discuss these points in more detail.

3.1 Unique factors

The UNIX system on the larger models of System/370 line, such as the IBM 3081K, increases by

over an order of magnitude the scale and scope that the operating system must manage. Numbers of pro-

cesses, I/O buffers, file descriptors, i-nodes, and other system resources are measured in hundreds or thou-

sands rather than tens or hundreds as on minicomputers.

One of the earliest concerns about a UNIX system implementation for large processors was its ability

to "scale"; that is, were there inherent characteristics of the UNIX system and its algorithms that limited its

implementation on large machines? Happily, we found that in most cases the straightforward algorithms

that implement the resource policies of the UNIX system perform quite well on this scale, leading one to

question the complex algorithms more typically employed in large operating systems. In a few cases the

standard algorithm was replaced for efficiency; for example, the standard UNIX system linear search of the

block buffers was replaced by a faster search based on hashing. The major area where scale appears to have

altered the character of the UNIX system is that of resource limitations on individual users or processes.

The impact of looping processes and file space consumers is more widespread, and the cause is more

- 7 -

elusive than in smaller systems. Efforts to detect and correct these types of problems have substantial bene-

fits in the System/370 environment.

Additional resources available on a mainframe, such as multiple central processors, powerful

autonomous I/O channels, fast peripherals such as drums and solid-state mass stores, large amounts of main

storage, and communications front-end processors greatly enhance the throughput of the UNIX system. In

particular, the dramatic increase in I/O bandwidth coupled with the use of ample main storage for the disk

block cache avoids the I/O-bound behavior typical of smaller UNIX systems. The increased main storage

and efficient paging capability increase the number of dispatchable processes and reduce idle time. The

front-end communication processors buffer the central processor(s) from character at a time I/O unless

required by the application (the so-called raw mode).

A number of adaptations of the UNIX system that take advantage of the characteristics of the main-

frame also enhance performance. The larger block size used (4096 bytes versus 512 or 1024 bytes in

smaller machines) reduces the overhead in I/O activities. To avoid the dramatic loss of usable space that

small files and directories would cause with 4096-byte blocks, the concept of large-block/small-block files

was introduced. Files of less than 493 bytes are stored directly in the corresponding i-node. As a side effect,

once the i-node for a small block file is read, no further disk access is required to retrieve the file contents.

This proves to be particularly beneficial for shell scripts, which are commonly used and often quite small,

as well as for small directories. In keeping with the scale of the mainframe and the development being done

on them, the file size limit on System/370 is currently 16 megabytes. This reduces the need to create and

process multiple files in applications such as databases, which require very large files.

3.2 Performance trade-offs

As a result of the factors cited above, the typical performance tradeoffs on a System/370 machine are

different from those for the minicomputer UNIX systems on which most of the current UNIX system pro-

grams were developed. Many UNIX system programs make extensive use of temporary files for even mod-

est amounts of data. Some tools, such as the C compiler, were divided into multiple processes intercon-

nected by temporary files to work around memory limitations imposed by early UNIX system hosts such as

the PDP-11 computer. The increased I/O bandwidth and the fact that many small temporary files remain

fully in the disk block cache reduces the impact of the widespread use of temporary files, but in areas where

such files have been eliminated, the performance gains have been impressive. In general, a shift in empha-

sis from temporary files toward greater use of main memory takes advantage of the additional spectrum

available and allows the efficient paging mechanism to dynamically manage data that the programmer had

previously explicitly and statically managed. Despite the trend toward increased use of memory, the aver-

age process still requires less than 200 kilobytes of the 8-megabyte user space.

3.3 System capacity

To determine system capacity of the UNIX system on System/370 machines relative to minicomput-

ers such as the PDP-11/70, VAX-11/780, and 3B20S computers, a set of scripts of typical software devel-

opment command mixes were developed and applied to differing UNIX system configurations. Results

indicated that the IBM 3033AP configuration first put into production was equivalent to several VAX-11/

780 or PDP-11/70 systems. Tuning of the VAX, 3B20S, and System/370 computers has varied these ratios

over time, but the overall order of magnitude spread has been maintained. Use of the newer IBM 3081K

processor has increased capacity by 50 percent, and evolution to the IBM 3084Q promises larger gains. In

actual operation a single large system obtains further efficiencies over the equivalent number of smaller

systems in terms of networking, operation, and administration. In general, we have found that highly

processor-intensive work loads, or work loads requiring a lot of parallel file system I/O, run relatively better

on the large System/370 machine; work loads characterized by many short interactions, context switches,

and character-oriented I/O run relatively more poorly.

Typical operational parameters of an IBM 3033AP are 150 simultaneous users (upwards of 200 have

been observed), 600 active processes (upwards of 1000 have been observed), 90-percent CPU usage on

both processors, and 10- to 20-percent usage of the I/O channels.

- 8 -

IV. INITIAL APPLICATION

4.1 Porting the application software

In early 1981 a production UNIX system was running on an IBM 3033AP in the Bell Laboratories

Indian Hill Computation Center. The next step was to port the application software tools of the 5ESS

switch development environment from the PDP-11/70 computers to the 3033AP. Over 300 tools, written in

both C and shell command language, were identified and examined. After careful study, almost half of the

tools were found to be little-used and were eliminated as candidates for porting to the 3033AP. The C pro-

grams required recompiling to generate objects that would run on a 3033AP; in general, they complied

without problems. The shell scripts were carried over with almost no problems. Regression tests were used

on the various C compilers to test all the compiler, assembler, and loader functions, and other programs

were unit tested. System testing, which consisted primarily of generating the system software for the 5ESS

switch, was then done.

In general the porting went very smoothly, with only minor problems. To the application program

developer and user, the System/370 appeared to be the same as the UNIX system on the minicomputers that

they were using. The effort to port the application tools was small and again proved the strength and com-

puter independence of the UNIX operating system and the associated application programs.

4.2 User migration

After testing the UNIX operating system and the application software tools, the users were migrated

from the PDP-11/70 computers to the 3033AP. To avoid a significant impact on the development of the

5ESS switch, a gradual rather than a flash migration was selected. The 3033AP was networked into the

nine PDP-11/70s and appeared as the tenth system. This allowed moving a subset of the users to the

3033AP but required continuing the multicomputer procedures to generate the software for the 5ESS

switch. About 10 percent of the users were moved on a weekend every two weeks. This allowed the staff

that was in charge of the migrations to work with these users, identify any special needs, and solve the

small number of problems that came up with each group. The users experienced no problems with the use

of the new machine because they saw the same user interface as before. This allowed the migration to pro-

ceed without the cost of any user education or any lost time as the users learned the new system.

4.3 Reliability

The combination of complex hardware with an attached processor configuration and the Series/1

front-end processor plus the three software packages (IBM Resident Supervisor, UNIX System Supervisor,

and Series 1 Terminal Handler) all interacting initially produced an availability of 80 percent. Even with 80

percent availability the project made progress faster than ever with the addition of a large concentrated pro-

cessor. By the final migration the availability was improved to the 95-percent range. In the next six months

the availability was improved to the 97- to 98-percent range, where it has stabilized. This is the same range

as the mature TSS/370 operating system running on similar hardware. While there were some early prob-

lems, they were much less than we had ever experienced in transferring a project to a new operating system

and the reliability that is associated with very mature operating systems was reached more quickly than we

had ever experienced.

4.4 Multiple System/370 environment

As the development project for the 5ESS switch continued to grow, additional System/370 machines

were added to the environment. The multiple PDP-11/70 software was ported to the IBM environment, and

successful multimachine operation was again in place. The current environment includes IBM 3033AP,

3033UP, and 3081K systems. The first application of a IBM 3081K processor with approximately 50 per-

cent more throughput than the 3033AP was in early 1983. This new system was brought up with the UNIX

operating system and the applications tools with no changes. From the first day it displayed the reliability

of a mature system.

- 9 -

4.5 Experience summary

The UNIX operating system with the Programmer’s Workbench software has proven to be an excel-

lent system to support software development. Our experience in developing the software for the 5ESS

switch has shown that there is a limit to the size of a software project that can be supported on minicomput-

ers. Up to now the UNIX operating system was not available on the large mainframe computers that are

necessary to provide the computing resources needed by a large project. With moving the UNIX operating

system to System/376 class mainframe systems, large projects can now take advantage of the UNIX operat-

ing system and its tools.

V. CONCLUSIONS

The UNIX system for System/370 has now been in production service for over two years, primarily

in support of the development project for the 5ESS switch. The growth in the number of systems and the

diversity of the IBM processors used (3031AP, 3033U, 3033AP, 3081K, and 4341) both testify to the suc-

cess of the concept of a UNIX system implementation for mainframe computers. Several innovative fea-

tures of the System/370 implementation, such as the use of semaphores for process synchronization, have

been found useful in other UNIX system implementations.

The proposal to implement the UNIX system on a large mainframe computer was initially met with

some skepticism. This may have been in part a result of the "small is beautiful" argument, and the feeling

that operating systems for large mainframes were themselves necessarily large, complex, and difficult to

use. We hope that the System/370 implementation has helped to demonstrate that this is not true. The avail-

ability of the UNIX system on a large mainframe has again raised the issue of small versus large machines;

e.g., should an installation buy several small systems, or would one large mainframe be better? There is, in

fact, nothing inherently better about either large or small systems; the decision should be based on the

user’s requirements, the character of the work load, and the overall cost.

The UNIX system is the only operating system available that runs on everything from one-chip

microcomputers to the largest general-purpose mainframes. While this represents at least a two-orders-of-

magnitude range in power and capacity, functionally the environments are the same; most programs that

execute in one environment will execute in the other without change. The ability of the UNIX system to

gracefully span the range from microcomputers to high-end mainframes is a tribute to its initial design over

a decade ago and to its careful evolution.

REFERENCES

1. S. C. Johnson and D. M. Ritchie, "UNIX Time-Sharing S stem: Portability of C Programs and the

UNIX System," B.S.T.J., 57, No. 6 stem: 1978), pp. 2021-48.

2. IBM System/370 Principles of Operation, Ninth Edition (October 1981), GA22-7000-8, IBM Corpo-

ration.

3. W. B. Smith and F. T. Andrews, Jr., "No. 5 ESS - Overview," Bell Telephone Laboratories; Interna-

tional Switching Symposium, Montreal, Canada, September 1981.

4. T. A. Dolotta, R. C. Haight, and J. R. Mashey, "UNIX Time-Sharing System: The Programmer’s

Workbench," B.S.T.J., 57, No. 6 (July-August 1978), pp. 2177-2200.

5. IBM System/360 Time Sharing System: System Logic Summary, Third Edition (June 1970), GY28-

2009-2, IBM Corporation.